# Introduction

The logical components of MarFS are the FUSE daemon running on the interactive FTA(s) (File Transfer Agents), pftool running on the batch FTA(s), and the utility programs for managing and maintaining MarFS. At least one underlying MDFS (Meta-Data File-System). MarFS data can be stored directly into the MDFS, but, presumably, one will also want an object-storage system.

# Basics

We assume the following variables, in order to make these instructions generic:

* SRC = directory under which MarFS code will be checked out
* PFS = path of a mounted parallel file-system
* GPFS = same as PFS, assuming PFS is gpfs.
* PA2X = dir where Ron Croonenberg’s parser-tool will be installed
* AWS4C = dir where the LANL-extended version of the aws4c library is checked-out
* PF = dir where pftool is installed

Where we show environment-variables on the command-line, in instructions below, these can be set in the environment, instead.

# Create infrastructure

## directories, filesets, etc

The configuration created in 4.3.1 will include namespaces that refer to file-systems and directories, which must currently be created by hand.

For each namespace:

* create a file-set where the MD for this NS will live
* create a directory under the fileset, matching the ‘md\_path’ in the config.
* assign ownership (chown), and access (chmod) to the directory.
* touch the file matching the ‘fsinfo\_path’ in the config
* create a fileset (and perhaps subdir) matching ‘trash\_path’ in the config.

For the fuse-mount:

* create the directory where fuse will be mounted

## repositories

MarFS data-storage can use a variety of storage back-ends. Each one may require different kinds of configuration:

### DIRECT

DIRECT repos store all data directly into the MDFS. Therefore, nothing special is needed, after the MDFS has been created.

### SPROXYD (Scality)

For each SPROXYD repo, the following is needed, on every server that will serve sproxyd requests:

edit /etc/sproxyd.conf

* add a driver alias matching the associated MarFS repo-name
* give it a unique service-id
* select storage parameters (e.g. ARC schema for erasure-coding)

edit /etc/httpd/conf.g/\_scality/sproxyd.conf

* add a new line for each MarFS namespace that will come here
* the lines can all be identical, except for the namespace-name

restart associated services (may take a moment)

* service restart httpd
* service restart scality-sproxyd

# Install and build MarFS, and associated tools

## Install RESTful object-storage tools

* cd $AWS4C
* git clone [git@github.com:jti-lanl/aws4c.git](mailto:git@github.com:jti-lanl/aws4c.git)
* make
* create ~/.awsAuth, with unix-user:storage-user:storage-key

## Install parser tools

* cd $PA2X
* git clone [git@git.lanl.gov:rocr/PA2X.git](mailto:git@git.lanl.gov:rocr/PA2X.git)

## Install MarFS

* cd $SRC
* git clone [git@github.com:mar-file-system/marfs.git](mailto:git@github.com:mar-file-system/marfs.git)

### Prepare local configuration

* (The following also builds libconfig.a, and cmd-line tool ‘marfs\_config’)
* cd $SRC/common/configuration/src
* edit marfs\_cctest.cfg [create repos and namespaces]
* make clean
* make PARSE\_DIR=$PA2X [ BLUEPRINT=… ] [ CONFIG=… ]

### Build and mount a MarFS fuse client (as root)

* (The following also builds libmarfs.a)
* cd $SRC/fuse/src
* make LIBAWS4C=$AWS4C
* make mnt

## Install pftool

* cd $PF
* git clone [git@github.com:pftool/pftool.git](mailto:git@github.com:pftool/pftool.git)
* TBD …

# Monitoring / Debugging

## MarFS Fuse

Fuse currently writes voluminous logs to syslog. You must enable syslog before these logs will be used.

* service syslog-ng start

When fuse is healthy:

* ‘mount’ will show the mount-point
* ‘ps –elf | grep fuse’ will show (one instance of) marfs\_fuse
* /var/log/messages will show activity during interaction with the fuse mount

To unmount fuse (as root)

* cd $SRC/fuse/src
* make umnt

If the above doesn’t work (as root)

* cd $SRC/fuse/src
* make abort

To report bugs that are simple reproducible problems:

* tail –f /var/log/messages
* [do the thing that causes the problem]
* cut-and-paste the part of the log that appeared during the preceding step

If fuse crashes on some activity (as root)

* ulimit –c unlimited
* [mount fuse]
* cause the crash
* send the /core\* that was created